RESILIENT SPC LVT FLOORING SPEC SHEET & WARRANTY GUIDE
Construction:    Layered Plank Consisting of UV coating, wear layer, décor film, vinyl and IXPE backing
Overall Thickness:    5.5mm (nominal)
Wear Layer Thickness:    0.3mm (12 Mil)
Size:    Various
Locking System:    Click
Edge:    Micro Bevel
Backing:    Attached 1.5mm IXPE Back
Noise Control:    IIC: 65 / STC: 62
Gloss Level:    Matt
Use:    Residential, Commercial
Surface Texture:    Wood Grain Embossed 
Packing Carton Size:    Various
Pieces Per Carton:    10
HUD/FHA Requirements:   Exceeds
Warranty:    25 Years Residential, 5 Year Limited Light Commercial
Recycling:    Suitable

LIMITED 25 YEAR RESIDENTIAL WARRANTY
Aspen Spring Flooring warrants that its Resilient Flooring will be free from manufacturing defects and, for 25 years following the date
following the date of purchase, under normal household conditions , will not:
• Permanently indent
• Rip, tear or gouge
• Wear through the wear layer so that the printed pattern or design of the floor is altered
LIMITED 5 YEAR LIGHT COMMERCIAL WARRANTY
Aspen Spring Flooring warrants that its Resilient Flooring will be free from manufacturing defects and, for 5 years following the date
of purchase, under normal commercial use, will not:
• Permanently indent
• Rip, tear or gouge
• Wear through the wear layer so that the printed pattern or design of the floor is altered